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What's New in v1.02

	Improvement
	Details

	OS Compatibility
	Full support for Windows 7 (SP1), Windows 10, and Windows 11 — 32 & 64-bit.

	MEDC17 Checksum Fix
	Resolved checksum calculation errors on MEDC17 ECU read/write operations.

	USB Stability
	Improved reconnection logic — significantly reduces 'Connection Lost' occurrences.

	Driver Signing (SHA-256)
	Super Driver updated with valid Microsoft signatures for Win10/11 enforcement.

	Connection Lost Solution
	New bundled utility to disable USB sleep and manage antivirus/firewall for ECU sessions.

	Security Dongle Detection
	Faster dongle enumeration on USB 3.0 hubs; fallback to USB 2.0 protocol on legacy systems.



System Requirements

	Operating System
	Windows 7 SP1  ·  Windows 10  ·  Windows 11  (32-bit & 64-bit)

	USB
	Powered USB 2.0 or USB 3.0 hub (mandatory — direct port may cause instability)pacakge come with usb 2.0 hub

	RAM
	2 GB minimum  ·  4 GB recommended

	Storage
	500 MB free disk space for installer and firmware cache

	Permissions
	Administrator account required for driver installation and launch

	Security Dongle
	Must be connected to the same USB hub as the Padflash device at startup




Hardware Connection — Live Diagram

Connect all devices to the powered USB hub before launching any driver tool or Padflash V2.
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Step-by-Step Installation Procedure

Read all phases before starting. Complete steps in order — skipping any step may cause device connection failures.

	PHASE 1 — SOFTWARE UPDATE

	01
	Uninstall previous Padflash software
Control Panel → Programs & Features → Padflash → Uninstall

	02
	Install Padflash Updater
Run PadflashUpdater_Setup.exe with Administrator privileges

	03
	Update to Version 1.02
Open Padflash Updater → click Update → wait for full download

	04
	Download firmware & restart Updater
Confirm download completes, then close and reopen Padflash Updater

	PHASE 2 — HARDWARE & DRIVER SETUP

	05
	Connect Padflash device to USB Hub
Plug device USB cable into any port on the powered hub

	06
	Connect Security Dongle to USB Hub
Plug dongle into a separate port on the same powered hub

	07
	Run Super Driver as Administrator
Right-click superdriver.exe → Run as Administrator

	08
	Click Install Driver inside Super Driver
Wait for the success notification before continuing

	09
	Install driver via Padflash Driver Tool
Open Padflash Driver → Install → accept all prompts

	PHASE 3 — SYSTEM CONFIGURATION

	10
	Run Padflash Connection Lost Solution
Right-click the utility shortcut → Run as Administrator

	11
	Disable USB Sleep / Power Management
Click 'Disable USB Sleep' inside the tool → confirm

	12
	Acquire Administrator Rights
Click 'Gain Admin Rights' → allow UAC prompt

	13
	Disable Antivirus & Firewall
Click 'Disable AV & Firewall' — re-enable after testing

	PHASE 4 — FINAL LAUNCH

	14
	Reboot the computer
Full shutdown and cold restart — mandatory, do not skip

	15
	Open Padflash Updater after reboot
Confirm version 1.02 is shown in the title bar

	16
	Launch Padflash V2 as Administrator
Desktop icon → right-click → Run as Administrator → ready





Installation Flowchart
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Troubleshooting

	Symptom
	Recommended Action

	Device not detected
	Reconnect device and dongle to hub. Re-run Super Driver. Reinstall Padflash Driver.

	Connection Lost error
	Run Connection Lost Solution → Disable USB Sleep → Reboot.

	Driver install fails
	Temporarily disable Defender & antivirus. Always run Super Driver as Administrator.

	MEDC17 checksum error
	Ensure v1.02 is installed — the MEDC17 fix is exclusive to this release.

	Software won't launch
	Always right-click Padflash V2 → Run as Administrator.

	Windows 7 compatibility
	Ensure SP1 is installed. Run sfc /scannow from an admin command prompt if drivers fail.

	Dongle not recognized
	Connect dongle directly to the powered USB hub. Avoid extension cables.



Support

If issues persist after completing all steps, contact your authorized Padflash reseller with your device serial number and a screenshot of the error message.

Always launch Padflash V2 via Run as Administrator. Failure to do so is the leading cause of connection and licensing errors.
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